
3 POINT HITCH WOOD CHIPPER

MODELS: VC40
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INTRODUCTION
Congratulations on your choice of a 3 Point Hitch Wood Chipper to compliment your opera- tion. This equipment has been designed and manufactured to meet the needs of a discerning timber or landscaping industry.

Safe, efficient and trouble free operation of your  Wood Chipper requires that you and anyone else who will be using or maintaining the chipper, read and understand the Safety, Operation, Mainte- nance and Trouble Shooting information contained within the Operator's Manual.

This manual covers the 3 Point Hitch Wood Chipper BX42
Keep this manual handy for frequent reference and to pass on to new operators or owners. Call your  dealer or the Distributer if you need assistance, information or additional copies of the manu- als.

OPERATOR ORIENTATION - The directions left, right, front and rear, as mentioned throughout this manual, are determined when sitting in the tractor driver's seat and facing in the direction of travel. 
2
SAFETY


SAFETY ALERT SYMBOL
This Safety Alert symbol means ATTENTION!  BECOME ALERT! YOUR SAFETY IS INVOLVED!

The Safety Alert symbol identifies important safety messages on the 3 Point Hitch Wood Chipper and in the manual. When you see this symbol, be alert to
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the possibility of personal injury or death.  Follow the instructions in the safety message.

Why is SAFETY important to you?

3 Big Reasons

Accidents Disable and Kill
Accidents Cost
Accidents Can Be Avoided
SIGNAL WORDS:
Note the use of the signal words DANGER, WARNING and CAUTION with the safety messages. The appropriate signal word for each message has been selected using the

following guide-lines:


DANGER -   Indicates an imminently hazardous situation that, if not avoided, will result in death or serious injury. This signal word is to be limited to the most extreme situations typically for

machine components which, for func- tional purposes, cannot be guarded.

WARNING -  Indicates a potentially hazardous situation that, if not avoided, could result in death or serious injury, and includes hazards that are exposed when guards are removed. It may also be used to alert against unsafe practices.

CAUTION -  Indicates a potentially hazardous situation that, if not avoided, may result in minor or moderate injury.  It may also be used to alert against unsafe practices.

If you have any questions not answered in this manual or require additional copies or the manual is dam- aged, please contact your dealer [image: image7.png]g Al g}
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SAFETY
YOU are responsible for the SAFE operation and maintenance of your  3 Point Hitch Wood Chipper. YOU must ensure that you and anyone else who is going to use, maintain or work around the 3 Point Hitch Wood Chipper be famil- iar with the using and maintenance procedures and related SAFETY information contained in this manual. This manual will take you step-by-step through your working day and alerts you to all good safety practices that should be used while using the 3 Point Hitch Wood Chipper.

Remember, YOU are the key to safety. Good safety practices not only protect you but also the people around you. Make these practices a work- ing part of your safety program.  Be certain that EVERYONE using this equipment is familiar with the recommended using and maintenance proce- dures and follows all the safety precautions. Most accidents can be prevented.  Do not risk injury or death by ignoring good safety practices.

•
3 Point Hitch Wood Chipper owners must give operating instructions to operators or em- ployees before allowing them to operate the machine, and at least annually thereafter.

•
The most important safety device on this equipment is a SAFE operator.  It is the op- erator’s responsibility to read and understand ALL Safety and Operating instructions in the manual and to follow these. Most accidents can be avoided.

•
A person who has not read and understood all

using and safety instructions is not qualified to use the machine. An untrained operator exposes himself and bystanders to possible serious injury or death.

•
Do not modify the equipment in any way.

Unauthorized modification may impair the function and/or safety and could affect the life of the equipment.

•
Think SAFETY! Work SAFELY!


2. 
GENERAL SAFETY
1.   Read and understand the Op- erator’s Manual and all safety signs before using, maintain- ing, adjusting or cleaning the

3 Point Hitch Wood Chipper.

2.   Have a first-aid kit available for use should the need arise and know how to use it.
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3.   Have a fire extinguisher available for use should the need arise and know how to use it.

4.   Do not allow riders.

5.   Wear appropriate protective gear. This list includes but is not limited to:

-
A hard hat

-
Protective shoes with slip

resistant soles

-
Protective glasses, goggles or face shield

-
Heavy gloves

-
Wet weather gear

-
Hearing Protection

-
Respirator or filter mask
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6.   Install and secure all guards before starting.

7.   Wear suitable ear protection for prolonged exposure to excessive noise.

8.   Turn machine off, stop and

disable engine, remove ignition key and place in your pocket, set park brake and wait for all moving parts to stop before servicing, adjust- ing, repairing or unplugging.

9.   Clear the area of people, especially small children, before using the unit.

10. Review safety related items annually with all personnel who will operating or maintaining the 3 Point Hitch Wood Chipper.

2.2
EQUIPMENT SAFETY GUIDELINES
1.   Safety of the operator and bystanders is one of the main concerns in designing and de- veloping equipment. However, every year many accidents occur which could have been avoided by a few seconds of thought and a more careful approach to handling equipment. You, the operator, can avoid many accidents by observing the following precautions in this section. To avoid personal injury or death, study the following precautions and insist those working with you, or for you to follow them.

2.   In order to provide a better view, certain photographs or illustrations in this manual may show an assembly with a safety shield removed.  However, equipment should never be used in this condition. Keep all shields in place.  If shield removal becomes necessary for repairs, replace the shield prior to use.

3.   Replace any safety sign or instruction sign that is not readable or is missing.  Location of such safety signs is indicated in this manual.

4.   Never use alcoholic beverages or drugs which can hinder alertness or coordination while us- ing this equipment. Consult your doctor about using this machine while taking prescription medications.

5.   Under no circumstances should young children be allowed to work with this equipment.  Do not allow persons to use or assemble this unit until they have read this manual and have developed a thorough understanding of the safety precautions and of how it works. Review the safety instructions with all users annually.

6.   This equipment is dangerous to children and persons unfamiliar with its operation. The operator should be a responsible, properly trained and physically able person familiar

with machinery and trained in this equipment's operations.  If the elderly are assisting with work, their physical limitations need to be recognized and accommodated.


7.   Never exceed the limits of a piece of machin- ery. If its ability to do a job, or to do so safely, is in question - DON'T TRY IT.
8.   Do not modify the equipment in any way.  Un- authorized modification may result in serious injury or death and may impair the function and life of the equipment.

9.   In addition to the design and configuration of this implement, including Safety Signs and Safety Equipment, hazard control and ac- cident prevention are dependent upon the awareness, concern, prudence, and proper training of personnel involved in the operation, transport, maintenance, and storage of the machine.  Refer also to Safety Messages and operation instruction in each of the appropri- ate sections of the tractor and machine manu- als. Pay close attention to the Safety Signs affixed to the tractor and the machine.

2.3
SAFETY TRAINING
1.   Safety is a primary concern in the design and manufacture of our products.  Unfortunately, our efforts to provide safe equipment can

be wiped out by a single careless act of an operator or bystander.

2.   In addition to the design and configuration of equipment, hazard control and accident pre- vention are dependent upon the awareness, concern, prudence and proper training of personnel involved in the operation, transport, maintenance and storage of this equipment.
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3.   It has been said, "The best safety feature is an informed, careful opera- tor." We ask you to be that

kind of an operator. It is the

operator's responsibility to read and under-

stand ALL Safety and Using instructions in the manual and to follow these. Accidents can be avoided.

4.   Working with unfamiliar equipment can lead to careless injuries. Read this manual before assembly or using, to acquaint yourself with the machine.  If this machine is used by any person other than yourself, or is loaned or rented, it is the machine owner's responsibility to make certain that the operator, prior to using:
a.   Reads and understands the operator's manuals.
b.   Is instructed in safe and proper use.
5.   Know your controls and how to stop tractor and machine quickly in an emergency.  Read this manual and the one provided with tractor.

6.   Train all new personnel and review instruc- tions frequently with existing workers.  Be certain only a properly trained and physically able person will use the machinery. A person who has not read and understood all using and safety instructions is not qualified to use the machine. An untrained operator exposes himself and bystanders to possible serious in- jury or death.  If the elderly are assisting with the work, their physical limitations need to be recognized and accommodated.


2.4
SAFETY SIGNS
1.   Keep safety signs clean and legible at all times.

2.   Replace safety signs that are missing or have become illegible.

3.   Replaced parts that displayed a safety sign should also display the current sign.

4.   Safety signs displayed in Section 3 each have a part number in the lower right hand corner. Use this part number when ordering replace- ment parts.

5.   Safety signs are available from your author- ized Distributor or Dealer Parts Department or the factory.

How to Install Safety Signs:
•
Be sure that the installation area is clean and dry.

•
Be sure temperature is above 50°F (10°C).

•
Determine exact position before you remove the backing paper.

•
Remove the smallest portion of the split back- ing paper.

•
Align the sign over the specified area and carefully press the small portion with the ex- posed sticky backing in place.

•
Slowly peel back the remaining paper and carefully smooth the remaining portion of the sign in place.

•
Small air pockets can be pierced with a pin and smoothed out using the piece of sign backing paper.

2. 
PREPARATION
1.   Never use the machine until you have read and completely understand this manual, the tractor Operator's Manual and each of the Safety Messages found on the safety signs on the tractor and machine.
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2.   Personal pro- tection equip- ment including hard hat, safety glasses, safety shoes, and gloves are rec- ommended dur- ing assembly,

installation, operation, adjustment, maintain- ing, repairing, removal, cleaning, or moving the unit.  Do not allow long hair, loose fitting clothing or jewellery to be around equipment.
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3.   PROLONGED EXPOSURE TO LOUD NOISE MAY CAUSE PERMANENT HEARING LOSS!
Power equipment with or without equipment attached can often be noisy enough to cause permanent, partial

hearing loss.  We recommend that you wear

hearing protection on a full-time basis if the noise in the Operator's position exceeds 80db. Noise over 85db on a long-term basis can cause severe hearing loss. Noise over 90db adjacent to the Operator over a long-term ba- sis may cause permanent, total hearing loss. NOTE:  Hearing loss from loud noise (from tractors, chain saws, radios, and other such sources close to the ear) is cumulative over a lifetime without hope of natural recovery.

4.   Clear working area of stones, branches or hidden obstacles that might be hooked or snagged, causing injury or damage.

5.   Use only in daylight or good artificial light.

6.   Be sure machine is properly mounted, adjust- ed and in good operating condition.

7.   Ensure that all safety shielding and safety signs are properly installed and in good condi- tion.


2.6
MAINTENANCE SAFETY
1.   Good maintenance is your responsibility. Poor maintenance is an invitation to trouble.

2.   Follow good shop practices.
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- Keep service area clean and dry.

- Be sure electrical outlets and tools are properly grounded.

- Use adequate light for the job at hand.

3.   Make sure there is

plenty of ventilation. Never operate the en- gine of the towing vehicle in a closed building. The exhaust fumes may cause asphyxiation.

4.   Before working on this machine, shut off the engine, set the brake, and turn fuel valve off.

5.   Never work under equipment unless it is blocked securely.

6.   Always use personal protection devices such as eye, hand and hearing protectors, when performing any service or maintenance work. Use heavy or leather gloves when handling blades.

7.   Where replacement parts are necessary for periodic maintenance and servicing, genuine factory replacement parts must be used to restore your equipment to original specifica- tions. The manufacturer will not be responsi- ble for injuries or damages caused by use of unapproved parts and/or accessories.

8.   A fire extinguisher and first aid kit should be
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kept readily accessible while performing main- tenance on this equipment.

9.   Periodically tighten all bolts,

nuts and screws and check that all electrical and fuel connections are properly secured to ensure unit is in a safe condition.

10. When completing a maintenance or service function, make sure all safety shields and devices are installed before placing unit in service.

2.  OPERATING SAFETY
1.   Please remember it is important that you read and heed the safety signs on the 3 Point Hitch Wood Chipper. Clean or replace all safety signs if they cannot be clearly read and under- stood. They are there for your safety, as well as the safety of others. The safe use of this machine is strictly up to you, the operator.

2.   All things with moving parts are potentially hazardous. There is no substitute for a cau- tious, safe-minded operator who recognizes potential hazards and follows reasonable safety practices. The manufacturer has designed this 3 Point Hitch Wood Chipper to be used with all its safety equipment properly attached, to minimize the chance of accidents. Study this manual to make sure you have all safety equipment attached.

3.   Close and secure rotor cover before operat- ing.

4.   Close and secure all guards, deflectors and

shields before starting and operating.

5.   Read and understand operator's manual before starting. Review safety instructions annually.

6.   Personal protection equipment including hear- ing protection, hard hat, safety glasses, safety shoes, and gloves are recommended during assembly, installation, operation, adjustment, maintaining, repairing, removal, or moving.

Do not allow long hair, loose-fitting clothing, or

jewellery to be around moving parts.

7.   Keep hydraulic lines and fittings tight, in good

condition and free of leaks.

8.   Never place any part of your body where it would be in danger if movement should occur during assembly, installation, operation, main- tenance, repairing, unplugging or moving.

9.   Turn machine off, stop and disable engine, remove ignition key and place in your pocket, set park brake and wait for all moving parts to stop before servicing, adjusting, repairing or unplugging.

10. Do not run machine inside a closed building to prevent asphyxiation from engine exhaust.



11. Use care when feeding material into chipper.

Do not send metal, bottles, cans, rocks, glass or other foreign material into wood chipper.  If foreign material enters chipper, stop machine, turn engine off and place ignition key in your pocket and wait for all moving parts to stop before removing material and/or unplugging. Inspect machine for damaged or loose parts before resuming work.

12. Never use alcoholic beverages or drugs which can hinder alertness or coordination while operating this equipment. Consult your doc- tor about operating this machine while taking prescription medications.

13. Do not allow riders on this machine at any time. There is no safe place for any riders.

14. Never allow children or unauthorized people to operate or be around this machine.

15. Do not reach into rotor or feed hopper open- ings when the engine is running.  Install and secure access covers before starting engine.

16  Keep the working area clean and free of de- bris to prevent tripping. Operate only on level ground.

17  Do not point discharge at people, animals or buildings.  Rotor can expel wood chips fast enough to cause injury.

18. Do not move or transport chipper when the rotor is turning.

19. Do not exceed a safe travel speed when transporting.
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3
SAFETY SIGN LOCATIONS
The types of safety signs and locations on the equipment are shown in the illustrations that follow. Good safety requires that you familiarize yourself with the various safety signs, the type of warning and the area, or particular function related to that area, that requires your SAFETY AWARENESS.

•  Think SAFETY! Work SAFELY!

D
A
F B
A
B
Z9400 
Z94006
REMEMBER - If safety signs have been damaged, removed, become illegible or parts replaced without safety signs, new signs must be applied.  New safety signs are available from your authorized dealer.

The types of safety signs and locations on the equipment are shown in the illustrations that follow. Good safety requires that you familiarize yourself with the various safety signs, the type of warning and the area, or particular function related to that area, that requires your SAFETY AWARENESS.

B B
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DANGER
THROWN OBJECT HAZARD
To prevent serious injury or death from thrown objects:
•   Turn machine off, stop and disable en- gine, remove ignition key and place in your pocket, set park brake and wait for all moving parts to stop before adjusting, servicing, maintaining, repairing or un- plugging.
•   Do not direct discharge duct towards people, animals or property. Always wear appropriate safety gear. Keep hands and feet out of discharge openings.



Z940   3
•   Keep others away.


Z9400 
[image: image22.png]* Read and understand operator’s manual before
starting. Review safety instructions annually.

» Turn machine off, stop and disable engine, re-
move ignition key and place in your pocket, set
park brake and wait for all moving parts to stop
before adjusting, servicing, maintaining, repairing or unplug-
ging.




REMEMBER - If safety signs have been damaged, removed, become illegible or parts replaced without safety signs, new signs must be applied.  New safety signs are available from your authorized dealer
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BX425/BX62S MAIN PARTS BREAKDOWN<
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BX42S/BX62S MAIN PARTS BREAKDOWN
	REF
	PART NUMBER
	DESCRIPTION
	NAME
	QTY

	
	BX42S
	BX62S
	BX42S
	BX62S
	BX42S
	BX62S
	

	1
	BX42S.1
	BX42R.4
	Assembly, Discharge Chute
	出料口总成
	1

	2
	BX42S.2
	BX62S.2
	Self-Feed Hopper
	加料斗总成
	1

	3
	BX42S-1
	BX62R.8
	Bracket, PTO Cover Mount
	托架
	1

	4
	BX42S-2
	BX62R.9
	PTO Cover
	PTO罩壳
	1

	5
	BX42S-3
	BX62R.3.2
	Knife, Rotor
	刀片
	4

	6
	BX42S-5
	BX62R.7
	Knife, Ledger
	定刀
	1

	7
	BX42S.3
	BX62S.1
	Housing, Bottom Rotor
	底座焊合件
	1

	8
	BX42S.4
	BX62R.5
	  
	上罩焊合件
	1

	9
	BX42S.5
	BX62R.3.1
	Rotor
	刀盘焊合件
	1

	10
	BX42S.6
	BX62R.6
	Twig Breaker
	侧刀焊合件
	1

	11
	Z11431
	Implement Pin
	悬挂销
	2

	12
	Z12110
	Latch Pin
	插销
	1

	13
	Z25204
	Z25203
	4-Bolt Bearing
	带座轴承F208
	带座轴承F210
	2

	14
	GB/T1152-89/M6
	Grease Zerk M6
	油杯M6
	2

	15
	Z44501
	05B-900
	#5 PTO Shaft M10 Shear
	PTO输出轴
	1

	16
	GB/T5783/M6x20
	GB/T5783/M10x20
	Bolt M6x20
	Bolt M10x20
	螺栓M6x20
	螺栓M10x20
	2

	17
	GB/T5783/M12x30
	GB/T5783/M12x35
	Bolt M12x30
	Bolt M12x35
	螺栓M12x30
	螺栓M12x35
	7

	18
	GB/T5786/M8x1x15
	GB/T5786/M12x1.5x25
	Bolt M8x1x15
	Bolt M12x1.5x25
	螺栓M8x1x15
	螺栓M12x1.5x25
	19

	19
	GB/T5786/M16x1.5x45
	Bolt M16x1.5x45
	螺栓M16x1.5x45
	8

	20
	GB/T889.1/M6
	GB/T889.1/M10
	Lock Nut M6
	Lock Nut M10
	锁紧螺母M6
	锁紧螺母M10
	2

	21
	GB/T93/22
	Lock washer 22
	弹簧垫圈22
	2

	22
	GB/T889.1/M12
	Lock Nut M12
	锁紧螺母M12
	5

	23
	GB/T6177.1/M10
	Flange Nut M10
	法兰螺母M10
	2

	24
	GB/T6171/22x1.5
	Nut M22 x1.5
	细牙螺母M22x1.5
	2

	25
	GB/T97.1/8
	GB/T97.1/12
	Plain washer 8
	Plain washer 12
	平垫圈 8
	平垫圈 12
	3

	26
	Z94601
	Z96605
	SMV Decal / Spade
	加料斗帖花
	1
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HOPPER/DISCHARGE CHUTE PARTS BREAKDOWN
	REF
	PART NUMBER
	DESCRIPTION
	NAME
	QTY

	
	BX42S
	BX62S
	BX42S
	BX62S
	BX42S
	BX62S
	

	1
	BX42S.1-1
	BX62R.4.3
	Plate, Spacer Ring
	隔片
	1

	2
	BX42S.1-2
	BX62R.4.3
	Plate, Spacer Ring
	隔片
	1

	3
	BX42S.1-3
	BX62R.4.4
	Plate, Hood Capture
	下夹片
	1

	4
	BX42S.1-4
	BX62R.4.2
	Deflector, Discharge Chute
	出料口罩
	1

	5
	BX42S.1-3
	BX62R.4.4
	Plate, Hood Capture
	下夹片
	1

	6
	BX42S.1.1
	BX62R.4.1
	Discharge Chute
	出料口焊合件
	1

	7
	1012W208
	Assembly, Hood Latch
	锁扣总成
	1

	8
	GB/T5783/M6x20
	Bolt M6x20
	螺栓M6x20
	8

	9
	GB/T889.1/M6
	Lock Nut M6
	锁紧螺母M6
	8

	10
	
	BX62R.4.5
	Spring 25mm x 178mm Heavy
	拉簧
	1

	11
	
	Z92304
	Single-Jack Chain #10 (35 links)
	链环
	35

	12
	Z19313
	JB/T8108.2
	Knob
	手柄
	2

	13
	GB/T802/M8
	
	Acorn Nut M8
	  盖形螺母M8
	
	2

	
	
	JB/T8108.2
	
	短环链3x1100
	
	

	REF
	PART NUMBER
	DESCRIPTION
	名称
	QTY

	
	BX42S
	BX62S
	BX42S
	BX62S
	BX42S
	BX62S
	

	20
	BX42S.2-1
	BX62R.2.16
	Strap, Hopper Flap
	压条
	1

	21
	BX42S.2.1
	BX62S.2-1
	Weldment, Infeed Hopper
	加料斗焊合件
	1

	22
	BX42S.2-2
	BX62R.2.15
	Flap, Hopper
	橡胶挡板
	2

	23
	GB/T889.1/M8
	GB/T889.1/M6
	Lock Nut M8
	锁紧螺母M8
	锁紧螺母M6
	3/4

	24
	GB/T12/M8x25
	GB/T5783/M6x20
	Carriage Bolt M8x25
	Bolt M6x20
	半圆头方颈螺栓M8x25
	螺栓M6x20
	3/4
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[image: image23.png]ping or tripping. Operate only on level ground.
- Close and secure rotor cover before operating.

« Close and secure a|l guards, deflectors and shields before
starting and operating.



[image: image24.png]- Do not point discharge at people, animals or buildings. Rotor
can expel wood chips fast enough to cause injury.

- Do not allow children, animals or unauthorized people into
working area.

- Do not run machine inside a closed building to prevent as-
phyxiation from engine exhaust.

+ Use care when feeding material into chipper. Do not send
metal, bottles, cans, rocks, glass or other foreign material
into wood chipper. If foreign material enters chipper, stop the
machine, turn engine off and place ignition key in your pocket
and wait for all moving parts to stop before removing material
and/or unplugging. Inspect machine for damaged or loose
parts before returning to work.

« Always wear P.P.E. (Personal Protective Equipment) such as
safety goggles and heavy gloves whenever operating ma-
chine.
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operation.

+ Do not move or transport chipper when the rotor is turning.



[image: image26.png]


[image: image27.png]


[image: image28.png]


[image: image29.png]


[image: image30.png]MISSING GUARD HAZARD



[image: image31.png]Close and secure all guards and shlelds
before operating.



_1326537254

