
3 POINT HITCH WOOD CHIPPER

MODELS: VC60-R
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	Model
	BX62RD

	Weight
	505KG

	Chipping Capacity
	150mm

	Chipper housing opening
	165mm*254mm

	No. of knifes
	4 pcs in rotor, and 1 pcs counter blade



	Rotor size
	762mm

	Feeding system
	Hydraulic feeder

	Hopper opening
	635mm*635mm

	Discharge Height


	1879mm

	Discharge Hood Rotation


	360 degree

	Tractor HP
	55-80HP

	Emergency stop for feeder
	3 pcs ( right side, left side, top side). Push by stop, pull by start
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INTRODUCTION
Congratulations on your choice of a 3 Point Hitch Wood Chipper to compliment your opera- tion. This equipment has been designed and manufactured to meet the needs of a discerning timber or landscaping industry.

Safe, efficient and trouble free operation of your  Wood Chipper requires that you and anyone else who will be using or maintaining the chipper, read and understand the Safety, Operation, Mainte- nance and Trouble Shooting information contained within the Operator's Manual.

This manual covers the 3 Point Hitch Wood Chipper BX42
Keep this manual handy for frequent reference and to pass on to new operators or owners. Call your  dealer or the Distributer if you need assistance, information or additional copies of the manu- als.

OPERATOR ORIENTATION - The directions left, right, front and rear, as mentioned throughout this manual, are determined when sitting in the tractor driver's seat and facing in the direction of travel. 
2
SAFETY


SAFETY ALERT SYMBOL
This Safety Alert symbol means ATTENTION!  BECOME ALERT! YOUR SAFETY IS INVOLVED!

The Safety Alert symbol identifies important safety messages on the 3 Point Hitch Wood Chipper and in the manual. When you see this symbol, be alert to

[image: image7.png]


the possibility of personal injury or death.  Follow the instructions in the safety message.

Why is SAFETY important to you?

3 Big Reasons

Accidents Disable and Kill
Accidents Cost
Accidents Can Be Avoided
SIGNAL WORDS:
Note the use of the signal words DANGER, WARNING and CAUTION with the safety messages. The appropriate signal word for each message has been selected using the

following guide-lines:


DANGER -   Indicates an imminently hazardous situation that, if not avoided, will result in death or serious injury. This signal word is to be limited to the most extreme situations typically for

machine components which, for func- tional purposes, cannot be guarded.

WARNING -  Indicates a potentially hazardous situation that, if not avoided, could result in death or serious injury, and includes hazards that are exposed when guards are removed. It may also be used to alert against unsafe practices.

CAUTION -  Indicates a potentially hazardous situation that, if not avoided, may result in minor or moderate injury.  It may also be used to alert against unsafe practices.

If you have any questions not answered in this manual or require additional copies or the manual is dam- aged, please contact your dealer [image: image8.png]g Al g}
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.

SAFETY
YOU are responsible for the SAFE operation and maintenance of your  3 Point Hitch Wood Chipper. YOU must ensure that you and anyone else who is going to use, maintain or work around the 3 Point Hitch Wood Chipper be famil- iar with the using and maintenance procedures and related SAFETY information contained in this manual. This manual will take you step-by-step through your working day and alerts you to all good safety practices that should be used while using the 3 Point Hitch Wood Chipper.

Remember, YOU are the key to safety. Good safety practices not only protect you but also the people around you. Make these practices a work- ing part of your safety program.  Be certain that EVERYONE using this equipment is familiar with the recommended using and maintenance proce- dures and follows all the safety precautions. Most accidents can be prevented.  Do not risk injury or death by ignoring good safety practices.

•
3 Point Hitch Wood Chipper owners must give operating instructions to operators or em- ployees before allowing them to operate the machine, and at least annually thereafter.

•
The most important safety device on this equipment is a SAFE operator.  It is the op- erator’s responsibility to read and understand ALL Safety and Operating instructions in the manual and to follow these. Most accidents can be avoided.

•
A person who has not read and understood all

using and safety instructions is not qualified to use the machine. An untrained operator exposes himself and bystanders to possible serious injury or death.

•
Do not modify the equipment in any way.

Unauthorized modification may impair the function and/or safety and could affect the life of the equipment.

•
Think SAFETY! Work SAFELY!


2. 
GENERAL SAFETY
1.   Read and understand the Op- erator’s Manual and all safety signs before using, maintain- ing, adjusting or cleaning the

3 Point Hitch Wood Chipper.

2.   Have a first-aid kit available for use should the need arise and know how to use it.
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3.   Have a fire extinguisher available for use should the need arise and know how to use it.

4.   Do not allow riders.

5.   Wear appropriate protective gear. This list includes but is not limited to:

-
A hard hat

-
Protective shoes with slip

resistant soles

-
Protective glasses, goggles or face shield

-
Heavy gloves

-
Wet weather gear

-
Hearing Protection

-
Respirator or filter mask
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6.   Install and secure all guards before starting.

7.   Wear suitable ear protection for prolonged exposure to excessive noise.

8.   Turn machine off, stop and

disable engine, remove ignition key and place in your pocket, set park brake and wait for all moving parts to stop before servicing, adjust- ing, repairing or unplugging.

9.   Clear the area of people, especially small children, before using the unit.

10. Review safety related items annually with all personnel who will operating or maintaining the 3 Point Hitch Wood Chipper.

2.2
EQUIPMENT SAFETY GUIDELINES
1.   Safety of the operator and bystanders is one of the main concerns in designing and de- veloping equipment. However, every year many accidents occur which could have been avoided by a few seconds of thought and a more careful approach to handling equipment. You, the operator, can avoid many accidents by observing the following precautions in this section. To avoid personal injury or death, study the following precautions and insist those working with you, or for you to follow them.

2.   In order to provide a better view, certain photographs or illustrations in this manual may show an assembly with a safety shield removed.  However, equipment should never be used in this condition. Keep all shields in place.  If shield removal becomes necessary for repairs, replace the shield prior to use.

3.   Replace any safety sign or instruction sign that is not readable or is missing.  Location of such safety signs is indicated in this manual.

4.   Never use alcoholic beverages or drugs which can hinder alertness or coordination while us- ing this equipment. Consult your doctor about using this machine while taking prescription medications.

5.   Under no circumstances should young children be allowed to work with this equipment.  Do not allow persons to use or assemble this unit until they have read this manual and have developed a thorough understanding of the safety precautions and of how it works. Review the safety instructions with all users annually.

6.   This equipment is dangerous to children and persons unfamiliar with its operation. The operator should be a responsible, properly trained and physically able person familiar

with machinery and trained in this equipment's operations.  If the elderly are assisting with work, their physical limitations need to be recognized and accommodated.


7.   Never exceed the limits of a piece of machin- ery. If its ability to do a job, or to do so safely, is in question - DON'T TRY IT.
8.   Do not modify the equipment in any way.  Un- authorized modification may result in serious injury or death and may impair the function and life of the equipment.

9.   In addition to the design and configuration of this implement, including Safety Signs and Safety Equipment, hazard control and ac- cident prevention are dependent upon the awareness, concern, prudence, and proper training of personnel involved in the operation, transport, maintenance, and storage of the machine.  Refer also to Safety Messages and operation instruction in each of the appropri- ate sections of the tractor and machine manu- als. Pay close attention to the Safety Signs affixed to the tractor and the machine.

2.3
SAFETY TRAINING
1.   Safety is a primary concern in the design and manufacture of our products.  Unfortunately, our efforts to provide safe equipment can

be wiped out by a single careless act of an operator or bystander.

2.   In addition to the design and configuration of equipment, hazard control and accident pre- vention are dependent upon the awareness, concern, prudence and proper training of personnel involved in the operation, transport, maintenance and storage of this equipment.
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3.   It has been said, "The best safety feature is an informed, careful opera- tor." We ask you to be that

kind of an operator. It is the

operator's responsibility to read and under-

stand ALL Safety and Using instructions in the manual and to follow these. Accidents can be avoided.

4.   Working with unfamiliar equipment can lead to careless injuries. Read this manual before assembly or using, to acquaint yourself with the machine.  If this machine is used by any person other than yourself, or is loaned or rented, it is the machine owner's responsibility to make certain that the operator, prior to using:
a.   Reads and understands the operator's manuals.
b.   Is instructed in safe and proper use.
5.   Know your controls and how to stop tractor and machine quickly in an emergency.  Read this manual and the one provided with tractor.

6.   Train all new personnel and review instruc- tions frequently with existing workers.  Be certain only a properly trained and physically able person will use the machinery. A person who has not read and understood all using and safety instructions is not qualified to use the machine. An untrained operator exposes himself and bystanders to possible serious in- jury or death.  If the elderly are assisting with the work, their physical limitations need to be recognized and accommodated.


2.4
SAFETY SIGNS
1.   Keep safety signs clean and legible at all times.

2.   Replace safety signs that are missing or have become illegible.

3.   Replaced parts that displayed a safety sign should also display the current sign.

4.   Safety signs displayed in Section 3 each have a part number in the lower right hand corner. Use this part number when ordering replace- ment parts.

5.   Safety signs are available from your author- ized Distributor or Dealer Parts Department or the factory.

How to Install Safety Signs:
•
Be sure that the installation area is clean and dry.

•
Be sure temperature is above 50°F (10°C).

•
Determine exact position before you remove the backing paper.

•
Remove the smallest portion of the split back- ing paper.

•
Align the sign over the specified area and carefully press the small portion with the ex- posed sticky backing in place.

•
Slowly peel back the remaining paper and carefully smooth the remaining portion of the sign in place.

•
Small air pockets can be pierced with a pin and smoothed out using the piece of sign backing paper.

2. 
PREPARATION
1.   Never use the machine until you have read and completely understand this manual, the tractor Operator's Manual and each of the Safety Messages found on the safety signs on the tractor and machine.

[image: image14.png]g Al g}

e e



2.   Personal pro- tection equip- ment including hard hat, safety glasses, safety shoes, and gloves are rec- ommended dur- ing assembly,

installation, operation, adjustment, maintain- ing, repairing, removal, cleaning, or moving the unit.  Do not allow long hair, loose fitting clothing or jewellery to be around equipment.
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3.   PROLONGED EXPOSURE TO LOUD NOISE MAY CAUSE PERMANENT HEARING LOSS!
Power equipment with or without equipment attached can often be noisy enough to cause permanent, partial

hearing loss.  We recommend that you wear

hearing protection on a full-time basis if the noise in the Operator's position exceeds 80db. Noise over 85db on a long-term basis can cause severe hearing loss. Noise over 90db adjacent to the Operator over a long-term ba- sis may cause permanent, total hearing loss. NOTE:  Hearing loss from loud noise (from tractors, chain saws, radios, and other such sources close to the ear) is cumulative over a lifetime without hope of natural recovery.

4.   Clear working area of stones, branches or hidden obstacles that might be hooked or snagged, causing injury or damage.

5.   Use only in daylight or good artificial light.

6.   Be sure machine is properly mounted, adjust- ed and in good operating condition.

7.   Ensure that all safety shielding and safety signs are properly installed and in good condi- tion.


2.6
MAINTENANCE SAFETY
1.   Good maintenance is your responsibility. Poor maintenance is an invitation to trouble.

2.   Follow good shop practices.
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- Keep service area clean and dry.

- Be sure electrical outlets and tools are properly grounded.

- Use adequate light for the job at hand.

3.   Make sure there is

plenty of ventilation. Never operate the en- gine of the towing vehicle in a closed building. The exhaust fumes may cause asphyxiation.

4.   Before working on this machine, shut off the engine, set the brake, and turn fuel valve off.

5.   Never work under equipment unless it is blocked securely.

6.   Always use personal protection devices such as eye, hand and hearing protectors, when performing any service or maintenance work. Use heavy or leather gloves when handling blades.

7.   Where replacement parts are necessary for periodic maintenance and servicing, genuine factory replacement parts must be used to restore your equipment to original specifica- tions. The manufacturer will not be responsi- ble for injuries or damages caused by use of unapproved parts and/or accessories.

8.   A fire extinguisher and first aid kit should be
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kept readily accessible while performing main- tenance on this equipment.

9.   Periodically tighten all bolts,

nuts and screws and check that all electrical and fuel connections are properly secured to ensure unit is in a safe condition.

10. When completing a maintenance or service function, make sure all safety shields and devices are installed before placing unit in service.

2.  OPERATING SAFETY
1.   Please remember it is important that you read and heed the safety signs on the 3 Point Hitch Wood Chipper. Clean or replace all safety signs if they cannot be clearly read and under- stood. They are there for your safety, as well as the safety of others. The safe use of this machine is strictly up to you, the operator.

2.   All things with moving parts are potentially hazardous. There is no substitute for a cau- tious, safe-minded operator who recognizes potential hazards and follows reasonable safety practices. The manufacturer has designed this 3 Point Hitch Wood Chipper to be used with all its safety equipment properly attached, to minimize the chance of accidents. Study this manual to make sure you have all safety equipment attached.

3.   Close and secure rotor cover before operat- ing.

4.   Close and secure all guards, deflectors and

shields before starting and operating.

5.   Read and understand operator's manual before starting. Review safety instructions annually.

6.   Personal protection equipment including hear- ing protection, hard hat, safety glasses, safety shoes, and gloves are recommended during assembly, installation, operation, adjustment, maintaining, repairing, removal, or moving.

Do not allow long hair, loose-fitting clothing, or

jewellery to be around moving parts.

7.   Keep hydraulic lines and fittings tight, in good

condition and free of leaks.

8.   Never place any part of your body where it would be in danger if movement should occur during assembly, installation, operation, main- tenance, repairing, unplugging or moving.

9.   Turn machine off, stop and disable engine, remove ignition key and place in your pocket, set park brake and wait for all moving parts to stop before servicing, adjusting, repairing or unplugging.

10. Do not run machine inside a closed building to prevent asphyxiation from engine exhaust.



11. Use care when feeding material into chipper.

Do not send metal, bottles, cans, rocks, glass or other foreign material into wood chipper.  If foreign material enters chipper, stop machine, turn engine off and place ignition key in your pocket and wait for all moving parts to stop before removing material and/or unplugging. Inspect machine for damaged or loose parts before resuming work.

12. Never use alcoholic beverages or drugs which can hinder alertness or coordination while operating this equipment. Consult your doc- tor about operating this machine while taking prescription medications.

13. Do not allow riders on this machine at any time. There is no safe place for any riders.

14. Never allow children or unauthorized people to operate or be around this machine.

15. Do not reach into rotor or feed hopper open- ings when the engine is running.  Install and secure access covers before starting engine.

16  Keep the working area clean and free of de- bris to prevent tripping. Operate only on level ground.

17  Do not point discharge at people, animals or buildings.  Rotor can expel wood chips fast enough to cause injury.

18. Do not move or transport chipper when the rotor is turning.

19. Do not exceed a safe travel speed when transporting.

   1、Main part
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	1、Main part
REF
	BX62RD
	DESCRIPTION
	NAME
	QTY

	1
	GB/T7810 
	  Bearing F210
	带座轴承F210
	2

	2
	GB/T97.1
	Washer 14
	平垫圈14
	8

	3
	GB/T93
	Spring washer 14
	弹簧垫圈14
	8

	4
	GB/T5786 
	Bolt M14*1.5*45
	螺栓M14x1.5x45
	8

	5
	BX62R.9
	PTO Cover
	PTO罩壳
	1

	6
	GB/T5783
	Bolt M10*20
	螺栓M10x20
	2

	7
	GB/T889.1
	Nut M10
	螺母M10
	2

	8
	BX62R.8
	Plate
	托架
	1

	9
	GB/T6171
	Bolt M22*1.5
	螺母M22x1.5
	2

	10
	GB/T93
	Spring washer 22
	弹簧垫圈22
	2

	11
	BX42S.5
	Low Pin
	下悬挂销
	2

	12
	FEL300.111
	Lock pin 12
	锁销12
	3

	13
	BX42R.6
	Top pin
	销轴（上悬挂销）
	1

	14
	GB/T5783
	Bolt M12*35
	螺栓M12x35
	7

	15
	GB/T5783
	Bolt M12*25
	螺栓M12x25
	1

	16
	GB/T97.1
	Washer 12
	平挡圈12
	4

	17
	GB/T889.1
	Nut M12
	螺母M12
	5

	18
	BX42R.2
	Hopper
	进料斗总成
	1

	19
	　
	Lock pin
	∅5锁销
	1　

	20
	BX42R.4
	Assembly, Discharge Chute
	出料口总成
	1

	21
	BX62R.5
	Top cover weldment
	上罩焊合件
	1

	22
	BX62R.3
	Fly wheel assemble
	刀盘装配
	1


	23
	　
	Cover bearing
	轴承座罩
	1

	24
	BX62R.10
	Gas spring
	气弹簧
	2

	25
	GB/T5783
	Bolt M12*30
	螺栓M12x30
	4

	26
	GB/T5783
	Bolt M8*65
	螺栓M8x65
	4

	27
	GB/T889.1
	Nut M8
	螺母M8
	4

	28
	BX62R.6
	Counter knife bracket
	侧刀焊合件
	1

	29
	GB/T93
	Spring washer 10
	弹簧垫圈10
	2

	30
	GB/T96.1
	Big washer 10
	大垫圈10
	4

	31
	BX62R.11
	Adjustment bolt
	定刀调节螺栓
	2

	32
	GB/T5786
	Bolt M12*1.5*40
	螺栓M12x1.5x40
	2

	33
	GB/T93
	Spring washer 12
	弹簧垫圈12
	2

	34
	GB/T96.1
	Big washer 12
	大垫圈12
	3

	35
	GB/T5786
	Bolt M12*1.5*30
	螺栓M12x1.5x30
	2

	36
	BX62R.7
	Counter knife
	定刀 
	1


2、Hopper
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                                   2、Hopper
	REF
	BX62RD
	DESCRIPTION
	名称
	QTY

	1
	GB/T7810
	Bearing UCP208
	带立式座轴承UCP208
	2

	2
	GB/T97.1
	Washer 16
	平垫圈16
	8

	3
	GB889.1
	Nut M16
	螺母M16
	4

	4
	BX62R.2.14
	Plate
	下辊防护板
	1

	5
	GB 889.1
	Nut M8
	螺母M8
	7

	6
	GB/T5783
	Bolt M8*20
	螺栓M8x20
	4

	7
	BX62R.2.2
	Down roller
	下辊焊合件
	1

	8
	GB/T889.1
	Nut M12
	螺母M12
	12

	9
	GB/T97.1
	Washer 12
	平垫圈12
	12

	10
	GB/T7810
	Bearing UCF208
	带立式座轴承UCF208
	2

	11
	GB/T5783
	Bolt M12*45
	螺栓M12x45
	12

	12
	BX62R.2.3
	Top Roller
	上辊焊合件
	1

	13
	BX62R.2.20
	Spring2
	拉簧2
	3

	14
	BX62R.2.17
	Ring for shaft
	轴端挡圈
	2

	15
	GB/T78 
	Bolt M6*8
	止动螺钉M6x8
	4

	16
	BX62R.2.5
	Right bracket
	右摆臂焊合件
	1

	17
	M6-6x4
	Connection
	锁母式接头（含油管）
	2

	18
	GB/T889.1
	Nut M8
	螺母M8 
	3

	19
	BX62R.2.10
	Drag hook
	拉钩
	4

	20
	GB/T97.1
	Washer 10
	平垫圈10
	9

	21
	BX62R.2.8
	Cover
	罩壳焊合件
	1

	22
	GB/T93
	Spring washer10
	弹簧垫圈10
	7

	23
	GB/T5782
	Bolt M10*110
	螺栓M10x110
	2

	24
	GB/T5782
	Bolt M10*160
	螺栓M10x160
	2

	25
	GB/T1152
	Grease nipple M6*1
	油杯M 6x1
	2

	26
	BX62R.2.1
	Hopper weldment
	料斗焊合件
	1

	27
	GB/T96.1
	Big washer 10
	大垫圈10
	2

	28
	GB/T889.1
	Nut M10
	螺母M10
	2

	29
	BX62R.2.6
	Handle 
	拉手装配
	1

	30
	GB/T889.1
	Nut M14
	螺母M14
	8

	31
	BX62R.2.9
	Adjustment bar
	调节手柄
	1

	32
	BX62R.2.11
	Pin for bearing
	轴承销
	1

	33
	GB/T276 
	Bearing 62804-2RS
	轴承61804-2RS
	2

	34
	BX62R.2.19
	Spring1
	拉簧1
	1

	35
	GB/T91
	Circlip 3.2*20
	开口销3.2x20
	1

	36
	GB /T6178
	Nut M14
	开槽螺母M14
	1

	37
	GB/T97.1
	Washer 14
	平垫圈14
	2

	38
	BX62R.2.12
	Bar
	阀芯连接杆
	1

	39
	BX62R.2.4
	Left bracket
	左摆臂焊合件
	1

	40
	BX62R.2.21
	Pin
	阀芯连接杆上销轴
	1

	41
	GB/T91
	Circlip 5*20
	开口销5x20
	2

	42
	BX62R.2.13
	Pin
	阀芯连接杆下销轴
	1

	43
	BX62R.2.18.1
	Oil pipe 1
	油管1（L=1000）
	2

	44
	BX62R.2.18.3
	Oil pipe 3
	油管3（L=300）
	1

	45
	ZT-L20E-0W
	Valve
	换向阀
	1

	46
	　
	M18*1.5
	M18x1.5-M27x1.5直接头
	4

	47
	GB/T5783
	Bolt M10*70
	螺栓M10x70
	3

	48
	GB/T93
	Spring washer 8
	弹簧垫圈8
	2

	49
	ET12L0MD
	Connection M18*1.5
	三通组合接头M18x1.5
	1

	50
	WEE12LR 1/2MD 
	Connection M18*1.5-G1/2
	弯通可调向接头M18x1.5-G1/2
	1

	51
	GB/T5783
	Bolt M8*70
	螺栓M8x70
	2

	52
	GB/T97.1
	Washer 8
	平垫圈8
	2

	53
	FCH-60
	Flow adjustment
	流量阀
	1

	54
	GE12LR1//ED
	Connection M18*1.5-G1/2
	接头M18x1.5-G1/2
	7

	55
	BX62R.2.18.4
	Oil pipe4
	油管4（L=3600）
	2

	56
	GB/T5862
	Connection G1/2
	快换接头G1/2
	2

	57
	BMR-200-2-A-D-N1
	Motor
	摆线马达
	2

	58
	BX62R.2.18.2
	Oil pipe 2
	油管2（L=700）
	1

	59
	GB/T5783
	Bolt M6*12
	螺栓M6x12
	4

	60
	GB/T93
	Spring washer 6
	弹簧垫圈6
	8

	61
	GB/T97.1
	Washer 6
	平垫圈6
	8

	62
	BX62R.2.7
	Cover
	透盖
	1

	63
	GB/T5783
	Bolt M16
	螺栓M16x55 
	4

	64
	BX62R.2.15
	Rubber
	橡胶挡板
	2

	65
	BX62R.2.16
	Plate
	压条
	1


 3. Discharge Chute
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                                    3. Discharge Chute
	REF
	BX62RD
	DESCRIPTION
	NAME
	QTY

	1
	BX62R.4.2
	Cover weldment
	出料口罩焊合件
	1

	2
	　
	Nut
	星形手柄螺母
	2

	3
	BX62R.4.5
	Spring 3
	拉簧3
	1

	4
	BX62R.4.1
	Assembly, Discharge Chute
	出料口焊合件
	1

	5
	BX42S.1.2
	Lock pin
	锁扣
	1

	6
	BX62R.4.3
	Bushing
	隔片
	1

	7
	BX62R.4.4
	Plate
	下夹片
	1

	8
	GB/T889.1
	Nut 6
	螺母6
	8

	9
	GB/T97.1 
	Washer 6
	垫圈6
	8

	10
	GB/T5783
	Bolt M6*25
	螺栓M6x25
	8

	11
	JB/T8108.2
	Chain 3*1100
	短环链3x1100
	1

	12
	JB/T8112
	D- Lock
	D形卸扣S-DW-1（M5）
	1


4.Fly Wheel 

[image: image6.jpg]



   4.Fly wheel 

	REF
	BX62RD
	DESCRIPTION
	NAME 
	QTY

	1
	BX62R.3.1
	Fly wheel weldment
	刀盘焊合件
	1

	2
	GB /T5783
	Bolt M12*30
	螺栓M12x30
	16

	3
	GB /T93
	Spring washer 12
	弹簧垫圈12
	16

	4
	GB /T97.1
	Washer 12
	平垫圈12
	16

	5
	BX62R.3.2
	Knife
	刀片
	4
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